? Worn Hagon Shocks.

Change in Stem Length, with damper load and weight

|  |  |  |  |
| --- | --- | --- | --- |
| Pre Load  | Shortest (firm) | Mid | Longest (soft) |
| Mk2a & ½ tank fuel | 10mm | 17mm | 24mm |
| Rider (195lbs) | 34mm | 36mm | 40mm |
| Rider & Pillion (189lbs) | 42mm | 49mm | 46mm |